|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **EVALUATION CRITERIA FOR CABLING** | | |  |  |  |
|  |  |  |  |  |  |
| **TENDERER\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** | |  |  |  |  |
|  |  |  |  |  |  |
|  | **Quality Criteria** | **Aspect Weigthing (A)** | **Marks Awarded (B)** | **Weighted Marks (AxB)** |  |
| **1** | Submitted procedures for cable installations | 20% |  | 0 |  |
| **2** | Submitted procedures for cable terminations | 20% |  | 0 |  |
| **3** | Submitted procedures for cable handling and storing | 15% |  | 0 |  |
| **4** | Relevant Experience and Capability | 20% |  | 0 |  |
| **5** | Submitted procedures for loading and unloading of cable drums | 15% |  | 0 |  |
| **6** | List of Tools. Test Certificate of crimping tools and continuity test equipment’s | 10% |  | 0 |  |
|  | **Score (%)** |  |  | 0,00% |  |
|  | **Total Minimum Threshold** | 70% |  | FAIL! |  |

## Manadatory Technical Evaluation Criteria

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Mandatory Technical Criteria Description** | **Reference to Technical Specification / Tender Returnable** | **Motivation for use of Criteria** |
|  | Relevant company experience | SANS10198 & 240-56030637 | Vital to execute the task |
|  | Procedures for Cable Terminations | SANS10198 & 240-64636794 | Vital to execute the task |
|  | Procedure for Cable Installation | SANS10198 & 240-56030637 | Vital to execute the task |
|  | Procedure for Loading and Unloading Cable Drums | SANS10198 & 240-56030637 | Vital to execute the task |
|  | Procedures for Cable Handling and Storing | SANS 10198 & 240-56030637 | Vital to execute the task |
|  | List of Tools. Test Certificate of crimping tools and continuity test equipment’s | SANS10198 & 240-56030637 | Vital to execute the task |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

## Qualitative Technical Evaluation Criteria

Table 3: Removing and Installing Power and Control Cables- Qualitative Technical Evaluation Criteria

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | Qualitative Technical Criteria Description | | Reference to Technical Specification / Tender Returnable | Criteria Weighting  (%) | Criteria Sub Weighting  (%) |
|  | Relevant company experience(Projects completed in past 5 years) | | SANS10198 & 240-56030637 | 20 |  |
|  | 1.1 | Number of projects | SANS10198 & 240-56030637 |  | 4 |
|  | 1.2 | Project Scopes and values | SANS10198 & 240-56030637 |  | 4 |
|  | 1.3 | C.V of qualified personnel | SANS10198 & 240-56030637 |  | 4 |
|  | 1.4 | Substation names and completion dates | SANS10198 & 240-56030637 |  | 4 |
|  | 1.5 | Client contact person and details | SANS10198 & 240-56030637 |  | 4 |
|  | Procedures for Cable Terminations | | SANS10198 & 240-56030637 | 20 |  |
|  | 2.1 | Handling of spare cores | SANS10198 & 240-56030637 |  | 8 |
|  | 2.2 | Ferrule numbering | SANS10198 & 240-56030637 |  | 8 |
|  | 2.3 | Total number of manpower dedicated to this project | SANS10198 & 240-56030637 |  | 4 |
|  | Procedure for Cable Installation | | SANS10198 & 240-56030637 | 20 |  |
|  | 3.1 | Yard stone handling | SANS10198 & 240-56030637 |  | 5 |
|  | 3.2 | Trench cover handling | SANS10198 & 240-56030637 |  | 5 |
|  | 3.3 | Cable Glanding | SANS10198 & 240-56030637 |  | 5 |
|  | 3.4 | Cable numbering | SANS10198 & 240-56030637 |  | 5 |
|  | Procedure for Loading and Unloading Cable Drums | | SANS10198 & 240-56030637 | 15 |  |
|  | 4.1 | Adequacy of procedure i.e. Lifting cable drums | SANS10198 & 240-56030637 |  | 15 |
|  | Procedures for Cable Handling and Storing | | SANS10198 & 240-56030637 | 15 |  |
|  | 5.1 | Adequacy of procedure i.e. Transportation, Rolling direction etc. | SANS10198 & 240-56030637 |  | 15 |
|  | Tools and equipment | | SANS10198 & 240-56030637 9 | 10 |  |
|  | 6.1 | Adequacy of tools and equipment. Test Certificate of crimping tools and continuity test equipments | SANS10198 & 240-56030637 |  | 10 |
|  |  |  |  | TOTAL: 100 |  |