**Confirmation of Last Bid submitted**

This declaration is to confirm the last bid of

(Company name) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ in the Reverse Auction Supply and delivery of plumbing spares for a period of three (3) years at kriel power station on an “as and when” required basis for the total basket of Goods excluding vat is:

R………………………….…………

This price is fixed and Delivery cost is included.

**Signature:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Name:** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ **Date:** \_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Designation:** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Company:** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Items:

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Item no.** | **Description** | | **Unit** | **Quantity** | **Unit Rate** | **Total Price** |
| 100 | **PLUMBING SPARES** | |  |  |  |  |
| 101 | 15 mm Diameter 90 Degree Bend | | Ea. | 250 |  |  |
| 102 | 15 Mm Diameter Straight Coupler | | Ea. | 250 |  |  |
| 103 | 15 Mm Diameter Tee Equal Copper To Copper Fittings | | Ea. | 250 |  |  |
| 104 | 15 Mm Diameter Union Coupler Copper To Copper Fittings | | Ea. | 250 |  |  |
| 105 | 15 Mm X G 1/2 Diameter Union Coupler Copper To Iron Female Fittings | | Ea. | 250 |  |  |
| 106 | 15 Mm Diameter Equal Crossover Copper To Copper Fittings | | Ea. | 250 |  |  |
| 107 | 15 Mm Diameter Full Crossover Copper To Copper Fittings | | Ea. | 250 |  |  |
| 108 | 15 Mm Diameter Return Bend Copper To Copper Fittings | | Ea. | 250 |  |  |
| 109 | 15 Mm Diameter Holder Bat For Copper Tubing | | Ea. | 250 |  |  |
| 110 | 15 Mm X G 1/2 Diameter Union Coupler Copper To Iron Male Fittings | | Ea. | 250 |  |  |
| 111 | 15 Mm X 15 Mm X 22mm Diameter Tee Reducing In Equally Reduced Copper To Copper Fittings | | Ea. | 250 |  |  |
| 112 | 15 Mm X G3/4 Elbow 90 Degree Reducing Copper To Male Iron Fittings | | Ea. | 250 |  |  |
| 113 | 15 Mm Diameter End Cap | | Ea. | 250 |  |  |
| 114 | 15 Mm X G1/2 Tap Connector Straight Copper To Female Iron Fittings | | Ea. | 250 |  |  |
| 115 | 15 Mm X G 1/2 Tap Connector Bent Copper To Female Iron Fittings | | Ea. | 250 |  |  |
| 116 | 15 Mm X G1/2 Elbow 90 Degree Copper To Male Iron Fittings | | Ea. | 250 |  |  |
| 117 | 15 Mm X G1/2 Elbow 90 Degree Copper To Female Iron Fittings | | Ea. | 250 |  |  |
| 118 | 15 Mm Diameter Elbow 90 Degree Street Copper To Copper Fittings | | Ea. | 250 |  |  |
| 119 | 15 Mm X G 3/4 Diameter Coupler Straight Reducing Copper To Female Iron Fittings | | Ea. | 250 |  |  |
| 120 | 15 Mm Diameter Elbow 45 Degree Copper To Copper Fittings | | Ea. | 250 |  |  |
| 121 | 22 Mm Diameter 90 Degree Bend | | Ea. | 250 |  |  |
| 122 | 22 Mm Diameter Straight Coupler | | Ea. | 250 |  |  |
| 123 | 22 Mm Diameter T Piece | | Ea. | 250 |  |  |
| 124 | 22 Mm Diameter Copper To Copper Male | | Ea. | 250 |  |  |
| 125 | 22 Mm Diameter Copper To Copper Female | | Ea. | 250 |  |  |
| 126 | 22 Mm Diameter Equal Crossover Copper To Copper Fittings | | Ea. | 250 |  |  |
| 127 | 22 Mm Diameter Full Crossover Copper To Copper Fittings | | Ea. | 250 |  |  |
| 128 | 22 Mm Diameter Return Bend Copper To Copper Fittings | | Ea. | 250 |  |  |
| 129 | 22 Mm Diameter Holder Bat For Copper Tubing | | Ea. | 250 |  |  |
| 130 | 22 Mm X G 3/4 Diameter Union Coupler Copper To Iron Male Fittings | | Ea. | 250 |  |  |
| 131 | 22 Mm X 22 Mm X 28mm Diameter Tee Reducing In Equally Reduced Copper To Copper Fittings | | Ea. | 250 |  |  |
| 132 | 22 Mm Diameter End Cap | | Ea. | 250 |  |  |
| 133 | 22 Mm X G3/4 Tap Connector Straight Copper To Female Iron Fittings | | Ea. | 250 |  |  |
| 134 | 22 Mm X G 3/4 Tap Connector Bent Copper To Female Iron Fittings | | Ea. | 250 |  |  |
| 135 | 22 Mm X G3/4 Elbow 90 Degree Copper To Male Iron Fittings | | Ea. | 250 |  |  |
| 136 | 22 Mm X G3/4 Elbow 90 Degree Copper To Female Iron Fittings | | Ea. | 250 |  |  |
| 137 | 22 Mm Diameter Elbow 90 Degree Street Copper To Copper Fittings | | Ea. | 250 |  |  |
| 138 | 22 Mm Diameter Elbow 45 Degree Copper To Copper Fittings | | Ea. | 250 |  |  |
| 139 | 22 Mm Coupler Straight Copper To Female Iron Fittings | | Ea. | 250 |  |  |
| 140 | 22 Mm Coupler Straight Copper To Male Iron Fittings | | Ea. | 250 |  |  |
| 141 | 22 Mm X22 Mm Coupler Straight Reducer Copper To Copper Fittings | | Ea. | 250 |  |  |
| 142 | 15mm Diameter Copper Pipes, 4m Long | | Ea. | 250 |  |  |
| 143 | 22mm Diameter Copper Pipes, 4m Long | | Ea. | 250 |  |  |
|  | | | | | | |
| 144 | **CONEX FITTINGS** | Ea. | |  |  |  |
| 145 | 15 Mm Diameter 90 Degree Bend Copper To Copper | Ea. | | 250 |  |  |
| 146 | 15 Mm X G3/4 Diameter Coupler Straight Reducing Copper To Female Iron Fittings | Ea. | | 250 |  |  |
| 147 | 15 Mm X G 3/4 Diameter 90 Degree Copper To Male Iron Fitting | Ea. | | 250 |  |  |
| 148 | 15 Mm X G 3/4 Diameter 90 Degree Copper To Female Iron Fitting | Ea. | | 250 |  |  |
| 149 | 15 Mm Diameter Stop End Compression | Ea. | | 250 |  |  |
| 150 | 15 Mm X G 1/2 Diameter Pillar Tap Adaptor Copper To Female Iron Fittings | Ea. | | 250 |  |  |
| 151 | 28 Mm X 15 Mm Diameter Reducer Multi Step Copper To Copper Fittings | Ea. | | 250 |  |  |
| 152 | 22 Mm X 15 Mm Diameter Reducer Single Step Copper To Copper Fittings | Ea. | | 250 |  |  |
| 153 | 15 Mm X 15 Mm X G 1/2 Tee Copper To Copper Female Iron Branch Fittings | Ea. | | 250 |  |  |
| 154 | 15 Mm X 15 Mm X G 1/2 Tee Copper To Copper Male Iron Branch Fittings | Ea. | | 250 |  |  |
| 155 | 15 Mm X G 1/2 X 15 Mm Tee Copper To Female Iron To Copper Run Equally Reduced Fittings | Ea. | | 250 |  |  |
| 156 | 15mm X 15 Mm X 22 Mm Tee Reducing Copper To Copper Fittings | Ea. | | 250 |  |  |
| 157 | 15 mm Diameter Straight Coupler | Ea. | | 250 |  |  |
| 158 | 15 mm Diameter T Equal Piece Copper To Copper To Copper Fittings | Ea. | | 250 |  |  |
| 159 | 15 mm Diameter 90 Degree Bend Copper To Male Iron Fitting | Ea. | | 250 |  |  |
| 160 | 15 mm X G1/2 Diameter 90 Degree Swivel Elbow Copper To Female Iron Fitting | Ea. | | 250 |  |  |
| 161 | 22 mm Diameter Coupler Straight Reducer Copper To Copper Fittings | Ea. | | 250 |  |  |
| 162 | 22 mm X G1 Diameter Coupler Straight Reducing Copper To Male Iron Fittings | Ea. | | 250 |  |  |
| 163 | 22 mm X G1 Diameter Coupler Straight Reducing Copper To Female Iron Fittings | Ea. | | 250 |  |  |
| 164 | 22 mm X G 1 Diameter 90 Degree Copper To Male Iron Fitting | Ea. | | 250 |  |  |
| 165 | 22 mm X G 3/4 Diameter 90 Degree Copper To Female Iron Fitting | Ea. | | 250 |  |  |
| 166 | 22 mm Diameter Stop End Compression | Ea. | | 250 |  |  |
| 167 | 22 mm X G 3/4 Diameter Pillar Tap Adaptor Copper To Female Iron Fittings | Ea. | | 250 |  |  |
| 168 | 35 mm X 22 Mm Diameter Reducer Multi Step Copper To Copper Fittings | Ea. | | 250 |  |  |
| 169 | 28 mm X 22 Mm Diameter Reducer Single Step Copper To Copper Fittings | Ea. | | 250 |  |  |
| 170 | 22 mm X 22 Mm X G 3/4 Tee Copper To Copper Female Iron Branch Fittings | Ea. | | 250 |  |  |
| 171 | 22 mm X 22 Mm X G 3/4 Tee Copper To Copper Male Iron Branch Fittings | Ea. | | 250 |  |  |
| 172 | 22 mm X G 3/4 X 22 Mm Tee Copper To Female Iron To Copper Run Equally Reduced Fittings | Ea. | | 250 |  |  |
| 173 | 22mm X 22 Mm X 28 Mm Tee Reducing Copper To Copper To Copper Fittings | Ea. | | 250 |  |  |
| 174 | Kwikflo Pressure Control Valve G3/4 F1 Inlet And Outlet And G1/2 F1 Expansion Outlet Max Inlet Pressure 2500 Kpa System Pressure 400 Kpa | Ea. | | 60 |  |  |
| 175 | Master Flow No 1400kpa Cobra | Ea. | | 60 |  |  |
| 176 | Master Flow Kit No 1400kpa Cobra | Ea. | | 60 |  |  |
| 177 | Master Flow No 2 100kpa Cobra | Ea. | | 60 |  |  |
| 178 | "Beta" Close Couple Ceramic Toilet Pan And Cistern | Ea. | | 75 |  |  |
| 179 | "Beta" Semi-Close Coupler Toilet Pan And Cistern | Ea. | | 75 |  |  |
| 180 | Plastic White Double Flap Toilet Seats | Ea. | | 75 |  |  |
| 181 | "Beta" Valve Complete Parker 411-02002  LL-BIDO | Ea. | | 75 |  |  |
| 182 | Urinal Flat Back Vaal 0010 | Ea. | | 30 |  |  |
| 183 | Flush Master Jnr Urinal Valve Fj 6000 | Ea. | | 60 |  |  |
| 184 | Urinal Tail Pipe FJT 55 | Ea. | | 60 |  |  |
| 185 | Vac Break 111 Vacuum Breaker - Single Jumper 15 Mm C X C | Ea. | | 60 |  |  |
| 186 | Vac Break 111 Vacuum Breaker - Single Jumper 22 Mm C X C | Ea. | | 60 |  |  |
| 187 | 15 mm Diameter "Dutton" Float Valve | Ea. | | 60 |  |  |
| 188 | 15 mm Diameter Stilflo Valve | Ea. | | 60 |  |  |
| 189 | 15 mm Diameter Tap Jumper | Ea. | | 150 |  |  |
| 190 | 22 mm Diameter Tap Jumper | Ea. | | 150 |  |  |
| 191 | 38 mm Diameter "P"- Trap Rubber | Ea. | | 150 |  |  |
| 192 | 38 mm Diameter "S"- Trap Rubber | Ea. | | 60 |  |  |
| 193 | 19 Gram Butane Gas | Ea. | | 60 |  |  |
| 194 | 500 Ml UPVC Glue | Ea. | | 30 |  |  |
| 195 | Hemp For Galvanized Thread | Ea. | | 90 |  |  |
| 196 | 15 mm Diameter Chromium Plated Shower Rose | Ea. | | 60 |  |  |
| 197 | Latco (Twin Pack) 100 Kpa | Ea. | | 150 |  |  |
| 198 | 50 mm Diameter UPVC 90 Degree Bend | Ea. | | 150 |  |  |
| 199 | 50 mm Diameter UPVC Inspection Bend | Ea. | | 150 |  |  |
| 200 | 50 mm Diameter UPVC Straight Coupler | Ea. | | 150 |  |  |
| 201 | 50 mm Diameter UPVC T Piece | Ea. | | 150 |  |  |
| 202 | 50 mm Diameter 45 Degree UPVC Bend | Ea. | | 150 |  |  |
| 203 | Rubber Cones | Ea. | | 60 |  |  |
| 204 | 22 mm Diameter "Brass" Tap | Ea. | | 150 |  |  |
| 205 | G 3/4 Inlet X G 3/4 Outlet With Hose Union And Hose Tail Standard Brass | Ea. | | 60 |  |  |
| 206 | G 3/4 Stop Tap F1 X F1 Standard Brass | Ea. | | 60 |  |  |
| 207 | 11 Litre Plastic Toilet Cistern | Ea. | | 60 |  |  |
| 208 | Dual Flush Valve (FPDF) For Liquid Lever 1 And Solid Lever 2 | Ea. | | 60 |  |  |
| 209 | 15 Mm "Cobra" Basin Taps | Ea. | | 60 |  |  |
| 210 | 15 Mm Gala Basin Mixer One Hole Single Lever Mixer With Plug ,Chain And Mounting Kit | Ea. | | 30 |  |  |
| 211 | "Beta" Flush Arm Washer | Ea. | | 60 |  |  |
| 212 | 50 mm Diameter UPVC Pipe, 6m Long | Ea. | | 80 |  |  |
| 213 | Drain Cleaning Acid (1liter) | Ea. | | 150 |  |  |
| 214 | Silicone Sealer Clear Big Tube | Ea. | | 60 |  |  |
| 215 | 110 mm Diameter UPVC Pipe, 6m Long | Ea. | | 90 |  |  |
| 216 | 110 mm Diameter UPVC 90 Degree Bend | Ea. | | 60 |  |  |
| 217 | 110 mm Diameter UPVC 90 Degree Inspection Bend | Ea. | | 60 |  |  |
| 218 | 110 mm Diameter UPVC 90 Degree Bend With 50 Mm Inlet | Ea. | | 60 |  |  |
| 219 | 110 mm Diameter UPVC Straight Coupler | Ea. | | 60 |  |  |
| 220 | 110 mm Diameter UPVC Straight Coupler With 50 Mm Inlet | Ea. | | 160 |  |  |
| 221 | 110 mm Diameter UPVC Straight Coupler With Two 50 Mm Inlets | Ea. | | 60 |  |  |
| 222 | 110 mm Diameter UPVC Y Junction | Ea. | | 60 |  |  |
| 223 | 110 mm Diameter UPVC Inspection Eye | Ea. | | 60 |  |  |
| 224 | 110 mm Diameter Inspection Bend With Vent 50 | Ea. | | 150 |  |  |
| 225 | 110 mm To 50 Mm Diameter Reducer UPVC | Ea. | | 30 |  |  |
| 226 | "Courier" Ceramic White Bathroom Basin With Pedestal No Holes | Ea. | | 30 |  |  |
| 227 | 32mm Diameter Chromium Plated Basin Waste Fitting | Ea. | | 30 |  |  |
| 228 | 38mm Diameter Sink Waste Fitting | Ea. | | 30 |  |  |
| 229 | 75 mm Shower Waste With CP Shower Grating And RB Body | Ea. | | 60 |  |  |
| 230 | G 11/2 F1 Shower P Trap With Shallow Seal And CP Grating | Ea. | | 30 |  |  |
| 231 | 110 mm Diameter UPVC 45 Degree Bend | Ea. | | 30 |  |  |
| 232 | 200 L Kwikot Geyser | Ea. | | 20 |  |  |
| 233 | 150 L Kwikot Geyser | Ea. | | 30 |  |  |
| 234 | 50 L Kwikot Geyser | Ea. | | 30 |  |  |
| 235 | 2,5 Litre Hydro Boil Geyser | Ea. | | 30 |  |  |
| 236 | 5 Litre Hydro Boil Geyser | Ea. | | 30 |  |  |
| 237 | 7,5 Litre Hydro Boil Geyser | Ea. | | 30 |  |  |
| 238 | 10 Litre Hydro Boil Geyser | Ea. | | 20 |  |  |
| 239 | 15 Litre Hydro Boil Geyser | Ea. | | 20 |  |  |
| 240 | 25 Litre Hydro Boil Geyser | Ea. | | 20 |  |  |
| 241 | 15 mm Diameter Chromium Plated "Cobra" Swivel Sink Mixer | Ea. | | 50 |  |  |
| 242 | 15 mm Diameter "Cobra" Chromium Plated Sink Tap | Ea. | | 50 |  |  |
| 243 | 15 mm Diameter Chromium Plated Flexible Connector, 375 Mm Long | Ea. | | 60 |  |  |
| 244 | 900 mm Stainless Steel Single Sink | Ea. | | 20 |  |  |
| 245 | 1200 Stainless Steel Double Sink | Ea. | | 20 |  |  |
| 246 | Stainless Steel Prep Bowl. | Ea. | | 20 |  |  |
| 247 | Plumbing Solder Without Flux 500 Gram | Ea. | | 60 |  |  |
| 248 | Plumbing Flux | Ea. | | 30 |  |  |
| 249 | Poly Corp. Pipe 22mm X 100meter Roll | Ea. | | 30 |  |  |
| 250 | Poly Corp. Pipe 15mm X100 Meter Roll | Ea. | | 30 |  |  |
| 251 | 20mm Class 6 PVC Pipe 100 Meter Roll | Ea. | | 30 |  |  |
| 252 | 20mm 90 Degree PVC Bend | Ea. | | 90 |  |  |
| 253 | 20mm Straight Coupler PVC | Ea. | | 90 |  |  |
| 254 | 20mm “Tee” Piece PVC | Ea. | | 60 |  |  |
| 255 | 20mm Heavy Duty Water Clamps | Ea. | | 60 |  |  |
| 256 | Toilet Water Isolating Ball Valve ½” | Ea. | | 60 |  |  |
| 257 | Quick Flow Regulating Valve | Ea. | | 60 |  |  |
| 258 | 20mm PVC Class 6 Pipe 100meter Roll | Ea. | | 60 |  |  |
| 259 | Duel Top Flash Inner For Cistern | Ea. | | 60 |  |  |
| 260 | Hand Basin Cobra Mixer (Tap Hot And Cold Water) | Ea. | | 30 |  |  |
| 261 | True Fix Ceramic Basin Screws | Ea. | | 90 |  |  |
| 262 | H/D Drain Rod 2m Industrial Male And Female Ends | Ea. | | 30 |  |  |
|  |  |  | |  |  |  |
|  | **Total** |  | |  |  |  |