|  |  |  |
| --- | --- | --- |
| **To whom it may concern** | **Date** | **16 May 2025** |
| **Enquiries** | **Spha Madondo** |
| **E-mail address** | **Madondst@eskom.co.za** |

Dear Sir/Madam

|  |  |
| --- | --- |
| **Request for Enquiry Number** | **E1212CXMWP** |
| **Description / Project Title** | **Supply, delivery, installation, and commissioning of clarifier sludge level detection for cooling and raw water at Lethabo power station for a period of six (06) months** |
| **Tender Questions Closing Date** | **05 day before the closing date** |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item** | **Questions** | **Answers** | **Clarity Published Dates** |
| **1** | I kindly request that we coordinate a suitable date for conducting a site visit to the Lethabo Plant. This visit will allow us to assess operations and take precise measurements and align the next steps. | Non-compulsory site visit is scheduled as follows:  Date: 21 May 2025  Induction time: 10h00 (SAST)  Site walk Time: 11h00 to 12h00 (SAST)  Site address: Lethabo Power station  Tenderers must confirm their intention to attend with the Eskom Representative stating the name and surname, ID, Type of car and car registration of each proposed attendee**.** | 16 May 2025 |
| 2 | What is the depth of the clarifiers? | 45 m (CCW Clarifier) water depth: 6084 mm    23m (Raw Water Clarifier) water depth : 4340 mm | 16 May 2025 |
| 3 | Can the roll bolts be mounted on the wall? | Engaged the civil engineer and there should not be a problem in mounting the bracket to the inside of the pond. But we will need to approve whatever they want to mount before any work is carried out. But yes roll bolts and a bracket are fine for the costing purpose. |  |
| 4 | Who can we contact with regards to safety inductions? | The procurement officer will give directions at the award stage of the process. |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |